
What¡¯s New in NovaLCT-Mars V4.6.0


1. NovaLCT-Mars now supports A8 series receiving cards.

2. NovaLCT-Mars now supports 20 sets of data, detection of flat cables with symmetrical, triple and quadruple strips, and LED error detection.

3. New types of chip supported: MY9373, MY9348, MY9263, MBI5051B, MBI5253, MBI5353, SUM2035, SUM2135, SUM2117, SUM2131, SUM2033, SUM2130, ICN2038S, ICN2038A, ICN2053,SM16207,SM16017S, SM16159, ICN2038S, ICN2038A, ICN2053, SM16207, SM16017S, SM16159,     UCS9812, TLC59581

4. Data set exchange is more intelligent.

5. Fixed some of the known bugs.

Bug Fixes

1. Fixed an issue that monitoring reboots in specific situations.

2. Fixed a bug of abnormal error while screen configuration.
